ldns(3)

NAME
ldns_buffer2pkt_wire - convert buffer/wire format to ldns_pkt

SYNOPSIS
#include <stdint.h>
#include <stdbool.h>

#include <ldns/ldns.h>

ldns_status ldns_buffer2pkt_wire(ldns_pkt **packet, const ldns_buffer *buffer);

DESCRIPTION

ldns_buffer2pkt_wire() converts the data in the ldns_buffer (in wire format) to a DNS packet. This function will initialize and allocate memory space for the packet structure. .br packet: pointer to the structure to hold the packet .br buffer: the buffer with the data .br Returns LDNS_STATUS_OK if everything succeeds, error otherwise

AUTHOR
The ldns team at NLnet Labs.

REPORTING BUGS
Please report bugs to ldns-team@nlnetlabs.nl or in our bugzilla at http://www.nlnetlabs.nl/bugs/index.html

COPYRIGHT
Copyright (c) 2004 - 2006 NLnet Labs.

Licensed under the BSD License. There is NO warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.

SEE ALSO
perldoc Net::DNS, RFC1034, RFC1035, RFC4033, RFC4034 and RFC4035.

REMARKS
This manpage was automatically generated from the ldns source code.